# Guitar Tuner

## Méthode de téléversement
- USB

## Windows Installation

1) Windows WSL Binding

```sh
usbipd list
usbipd bind --busid 1-2
usbipd.exe attach --wsl --busid 1-2
```

2) Compile the code


```sh
make
```

3) Flash the code to the device

```sh
sudo make upload
```


## USB Descriptor

./.venv/bin/activate
python3 -M pip install pyusb
python3 receive.py
