SSD1306 OLED display driver 1.8.2 This library is developed to control SSD1306/SSD1331/SSD1351/IL9163/PCD8554 RGB i2c/spi LED displays

oled_sh1106.h
Go to the documentation of this file.
1 /*
2 MIT License
3
4 Copyright (c) 2017-2018, Alexey Dynda
5
6 Permission is hereby granted, free of charge, to any person obtaining a copy
7 of this software and associated documentation files (the "Software"), to deal
8 in the Software without restriction, including without limitation the rights
9 to use, copy, modify, merge, publish, distribute, sublicense, and/or sell
10 copies of the Software, and to permit persons to whom the Software is
11 furnished to do so, subject to the following conditions:
12
13 The above copyright notice and this permission notice shall be included in all
14 copies or substantial portions of the Software.
15
16 THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS OR
17 IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF MERCHANTABILITY,
18 FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL THE
19 AUTHORS OR COPYRIGHT HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER
20 LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING FROM,
21 OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR OTHER DEALINGS IN THE
22 SOFTWARE.
23 */
24
30 #ifndef _OLED_SH1106_H_
31 #define _OLED_SH1106_H_
32
33 #include "ssd1306_hal/io.h"
34
35 #ifdef __cplusplus
36 extern "C" {
37 #endif
38
50 void sh1106_128x64_init(void);
51
60 void sh1106_128x64_i2c_init(void);
61
70 void sh1106_128x64_spi_init(int8_t rstPin, int8_t cesPin, int8_t dcPin);
71
76 #ifdef __cplusplus
77 }
78 #endif
79
80 // ----------------------------------------------------------------------------
81 #endif // _OLED_SH1106_H_
sh1106_128x64_init
void sh1106_128x64_init(void)
Inits 128x64 OLED display (based on SH1106 controller).
Definition: oled_sh1106.c:97
io.h
sh1106_128x64_spi_init
void sh1106_128x64_spi_init(int8_t rstPin, int8_t cesPin, int8_t dcPin)
Inits 128x64 OLED display over spi (based on SH1106 controller).
Definition: oled_sh1106.c:119
sh1106_128x64_i2c_init
void sh1106_128x64_i2c_init(void)
Inits 128x64 OLED display over i2c (based on SH1106 controller).
Definition: oled_sh1106.c:113