SSD1306 OLED display driver 1.8.2 This library is developed to control SSD1306/SSD1331/SSD1351/IL9163/PCD8554 RGB i2c/spi LED displays

Classes
tiler.h File Reference
`#include "canvas.h"`
`#include "lcd/lcd_common.h"`

Go to the source code of this file.

## Classes
class | NanoEngineTiler< C, W, H, B >
#define | TILE_128x64_MONO NanoCanvas1, 128, 64, 7
| Full-screen 1-bit tile for SSD1306.
#define | TILE_8x8_MONO NanoCanvas1, 8, 8, 3
| Standard 1-bit tile 8x8 for monochrome mode.
#define | TILE_16x16_MONO NanoCanvas1, 16, 16, 4
| Standard 1-bit tile 16x16 for monochrome mode.
#define | TILE_32x32_MONO NanoCanvas1, 32, 32, 4
| Standard 1-bit tile 32x32 for monochrome mode.
#define | TILE_8x8_RGB8 NanoCanvas8, 8, 8, 3
| Standard 8-bit RGB tile 8x8.
#define | TILE_16x16_RGB8 NanoCanvas8, 16, 16, 4
| Standard 8-bit RGB tile 16x16.
#define | TILE_32x32_RGB8 NanoCanvas8, 32, 32, 5
| Standard 8-bit RGB tile 32x32.
#define | TILE_8x8_MONO_8 NanoCanvas1_8,8, 8, 3
| Standard 1-bit tile 8x8 for RGB mode.
#define | TILE_8x8_RGB16 NanoCanvas16, 8, 8, 3
| Standard 16-bit RGB tile 8x8.
#define | ADATILE_8x8_MONO AdafruitCanvas1, 8, 8, 3
| Use Adafruit GFX implementation as NanoEngine canvas.
#define | ADATILE_8x8_RGB8 AdafruitCanvas8, 8, 8, 3
| Use Adafruit GFX implementation as NanoEngine canvas.
#define | ADATILE_8x8_RGB16 AdafruitCanvas16, 8, 8, 3
| Use Adafruit GFX implementation as NanoEngine canvas.
typedef bool(* | TNanoEngineOnDraw) (void)
SFixedFontInfo | s_fixedFont

## Detailed Description

Tiler helper for graphics processing

Definition in file tiler.h.

## Typedef Documentation

## ◆ TNanoEngineOnDraw

typedef bool(* TNanoEngineOnDraw) (void)

Type of user-specified draw callback.

Definition at line 68 of file tiler.h.