SSD1306 OLED display driver 1.8.2 This library is developed to control SSD1306/SSD1331/SSD1351/IL9163/PCD8554 RGB i2c/spi LED displays

oled_ssd1351.h
Go to the documentation of this file.
1 /*
2 MIT License
3
4 Copyright (c) 2018, Alexey Dynda
5
6 Permission is hereby granted, free of charge, to any person obtaining a copy
7 of this software and associated documentation files (the "Software"), to deal
8 in the Software without restriction, including without limitation the rights
9 to use, copy, modify, merge, publish, distribute, sublicense, and/or sell
10 copies of the Software, and to permit persons to whom the Software is
11 furnished to do so, subject to the following conditions:
12
13 The above copyright notice and this permission notice shall be included in all
14 copies or substantial portions of the Software.
15
16 THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS OR
17 IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF MERCHANTABILITY,
18 FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL THE
19 AUTHORS OR COPYRIGHT HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER
20 LIABILITY, WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING FROM,
21 OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR OTHER DEALINGS IN THE
22 SOFTWARE.
23 */
29 #ifndef _OLED_SSD1351_H_
30 #define _OLED_SSD1351_H_
31
32 #include "ssd1306_hal/io.h"
33 #include "lcd/lcd_common.h"
34
35 #ifdef __cplusplus
36 extern "C" {
37 #endif
38
57 void ssd1351_setMode(lcd_mode_t mode);
58
67 void ssd1351_128x128_init(void);
68
77 void ssd1351_128x128_spi_init(int8_t rstPin, int8_t cesPin, int8_t dcPin);
78
83 #ifdef __cplusplus
84 }
85 #endif
86
87 // ----------------------------------------------------------------------------
88 #endif // _OLED_SSD1351_H_
ssd1351_setMode
void ssd1351_setMode(lcd_mode_t mode)
Sets GDRAM autoincrement mode.
Definition: oled_ssd1351.c:124
lcd_common.h
io.h
ssd1351_128x128_init
void ssd1351_128x128_init(void)
Inits 128x128 RGB OLED display (based on SSD1351 controller).
Definition: oled_ssd1351.c:184
lcd_mode_t
lcd_mode_t
Definition: lcd_common.h:69
ssd1351_128x128_spi_init
void ssd1351_128x128_spi_init(int8_t rstPin, int8_t cesPin, int8_t dcPin)
Inits 128x128 RGB OLED display over spi (based on SSD1351 controller).
Definition: oled_ssd1351.c:216