SSD1306 OLED display driver 1.8.2 This library is developed to control SSD1306/SSD1331/SSD1351/IL9163/PCD8554 RGB i2c/spi LED displays

Classes | Macros | Functions
ssd1306_generic.h File Reference
`#include "nano_gfx_types.h"`

Go to the source code of this file.

## Classes
struct | SAppMenu

## Macros
#define | SSD1306_MORE_CHARS_REQUIRED 0xffff

## Functions
void | ssd1306_setPos (uint8_t x, uint8_t y)
void | ssd1306_setCursor (lcdint_t x, lcdint_t y)
| Sets cursor position for text mode print functions. More...
void | ssd1306_setFixedFont (const uint8_t *progmemFont)
void | ssd1306_setFreeFont (const uint8_t *progmemFont)
void | ssd1306_setSecondaryFont (const uint8_t *progmemUnicode)
void | ssd1306_setFont6x8 (const uint8_t *progmemFont) __attribute__((deprecated))
void | ssd1306_getCharBitmap (uint16_t ch, SCharInfo *info)
| returns char data for currently set (active) font. More...
void | ssd1306_enableUtf8Mode (void)
void | ssd1306_enableAsciiMode (void)
lcduint_t | ssd1306_getTextSize (const char *text, lcduint_t *height)
void | ssd1306_createMenu (SAppMenu *menu, const char **items, uint8_t count)
void | ssd1306_showMenu (SAppMenu *menu)
void | ssd1306_showMenu8 (SAppMenu *menu)
void | ssd1306_showMenu16 (SAppMenu *menu)
void | ssd1306_updateMenu (SAppMenu *menu)
void | ssd1306_updateMenu8 (SAppMenu *menu)
void | ssd1306_updateMenu16 (SAppMenu *menu)
uint8_t | ssd1306_menuSelection (SAppMenu *menu)
void | ssd1306_menuDown (SAppMenu *menu)
void | ssd1306_menuUp (SAppMenu *menu)
void | ssd1306_drawProgressBar (int8_t progress)
void | ssd1306_drawProgressBar8 (int8_t progress)

## Detailed Description

SSD1306 generic API functions

Definition in file ssd1306_generic.h.

## Macro Definition Documentation

## ◆ SSD1306_MORE_CHARS_REQUIRED

#define SSD1306_MORE_CHARS_REQUIRED 0xffff

Flag means that more chars are required to decode utf-8

Definition at line 43 of file ssd1306_generic.h.